{"text_format":"3","workbook":"xls","n_sheets":10,"sheets":["封2预算总价","表02工程项目造价汇总表","表03单项工程造价汇总表","表04单位工程造价汇总表","表05分部分项工程量清单与计价表","表06总价措施项目清单与计价表","表07单价措施项目清单与计价表","表10分部分项工程量清单综合单价分析表","表11单价措施项目清单综合单价分析表","表14人工、材料设备、机械汇总表"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"封2预算总价","index":0,"n_rows":16,"n_cols":12,"rows_kept":16,"merged":[[1,1,1,5],[1,6,1,9],[2,6,2,7],[2,8,2,10],[3,0,3,11],[4,0,4,1],[4,2,4,4],[4,5,4,7],[4,8,4,11],[5,0,5,1],[5,2,5,4],[5,5,5,7],[5,8,5,11],[6,1,6,4],[6,6,6,11],[7,1,7,4],[7,5,7,11],[8,1,8,4],[8,6,8,11],[9,1,9,4],[9,6,9,11],[10,1,10,11],[11,1,11,11],[12,1,12,4],[12,6,12,11],[13,6,13,7],[13,8,13,10],[15,6,15,11]],"flags":["formulas_cached_only"]}
["  封2"," "," "," "," "," "," ",null," ",null,null," "]
[" ","水仙药业会议室及办公室装修",{"$nulls":4},"工程",{"$nulls":4}," "]
[" "," "," "," "," "," "," ",null," ",null,null," "]
["预 算 总 价"]
["预算总价（小写）：",null,"63197.06元",null,null,"其中：甲供材料费",null,null,"0元"]
["        （大写）：",null,"陆万叁仟壹佰玖拾柒元零陆分",null,null,"其中：甲供材料费",null,null,"零元整"]
["招 标 人："," ",{"$nulls":3}," 造价咨询人："," "]
[" ","（单位盖章）",{"$nulls":3},"（单位盖章或资质专用章）"]
["法定代表人\n或其授权人："," ",{"$nulls":3}," 法定代表人\n 或其授权人："," "]
[" ","（签字或盖章）",{"$nulls":3}," ","（签字或盖章）"]
["造价工程师："," "]
[" ","（签字盖专用章）"]
["编制时间："," ",{"$nulls":3},"复核时间："," "]
[" "," "," "," "," "," "," ",null," ",null,null," "]
[]
[null," "," "," "," "," "," "]

{"sheet":"表02工程项目造价汇总表","index":1,"n_rows":9,"n_cols":4,"rows_kept":9,"merged":[[1,0,1,3],[2,0,2,2],[6,0,6,1]],"flags":["formulas_cached_only"]}
["  表2"," "," "," "]
["工程项目造价汇总表"]
["工程名称：水仙药业会议室及办公室装修",null,null,"第1页 共1页"]
["序号","单项工程名称","金额（元）","其中：\n安全文明施工费\n（元）"]
["1","三层会议室及办公室","25136.29","237.46"]
["2","六层会议室及办公室","38060.77","359.33"]
["合    计",null,"63197.06","596.79"]
[]
[null," "," "," "]

{"sheet":"表03单项工程造价汇总表","index":2,"n_rows":20,"n_cols":4,"rows_kept":20,"merged":[[1,0,1,3],[2,0,2,2],[7,0,7,1],[11,0,11,3],[12,0,12,2],[17,0,17,1]],"flags":["formulas_cached_only"]}
["  表3"," "," "," "]
["单项工程造价汇总表"]
["工程名称：三层会议室及办公室",null,null,"第1页 共2页"]
["序号","单位工程名称","金额（元）","其中：\n安全文明施工费\n（元）"]
[" "," "," "," "]
["1","土建单位工程","17783.42","168"]
["2","安装单位工程","7352.87","69.46"]
["合    计",null,"25136.29","237.46"]
[]
[null," "," "," "]
["  表3"," "," "," "]
["单项工程造价汇总表"]
["工程名称：六层会议室及办公室",null,null,"第2页 共2页"]
["序号","单位工程名称","金额（元）","其中：\n安全文明施工费\n（元）"]
[" "," "," "," "]
["1","土建单位工程","27858.9","262.95"]
["2","安装单位工程","10201.87","96.38"]
["合    计",null,"38060.77","359.33"]
[]
[null," "," "," "]

{"sheet":"表04单位工程造价汇总表","index":3,"n_rows":95,"n_cols":4,"rows_kept":95,"merged":[[1,0,1,3],[2,0,2,1],[2,2,2,3],[3,1,3,2],[4,1,4,2],[5,1,5,2],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,0,22,2],[26,0,26,3],[27,0,27,1],[27,2,27,3],[28,1,28,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,0,43,2],[47,0,47,3],[48,0,48,1],[48,2,48,3],[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[56,1,56,2],[57,1,57,2],[58,1,58,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[69,1,69,2],[70,1,70,2],[71,0,71,2],[75,0,75,3],[76,0,76,1],[76,2,76,3],[77,1,77,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[84,1,84,2],[85,1,85,2],[86,1,86,2],[87,1,87,2],[88,1,88,2],[89,1,89,2],[90,1,90,2],[91,1,91,2],[92,0,92,2]],"flags":["formulas_cached_only"]}
["  表4"," "," "," "]
["单位工程造价汇总表"]
["工程名称：三层会议室及办公室_土建单位工程",null,"第1页 共4页"]
["序号","汇  总  内  容",null,"金额（元）"]
[" "," ",null," "]
[" "," ",null," "]
["1","分部分项工程费",null,"16812.17"]
["1.1","门窗工程",null,"4006.47"]
["1.2","天棚工程",null,"12661.52"]
["1.3","油漆、涂料、裱糊工程",null,"93.27"]
["1.4","拆除工程",null,"50.91"]
["2","措施项目费",null,"971.25"]
["2.1","总价措施项目费",null,"228.88"]
["2.1.1","安全文明施工费",null,"168"]
["2.1.2","其他总价措施费",null,"19.31"]
["2.1.3","扬尘防治措施费",null,"20.5"]
["2.1.4","建筑工人实名制措施费",null,"21.07"]
["2.2","单价措施项目费",null,"742.37"]
["3","其他项目费",null,"0"]
["3.1","暂列金额",null,"0"]
["3.2","专业工程暂估价",null,"0"]
["3.3","总承包服务费",null,"0"]
["合计=1+2+3",null,null,"17783.42"]
[]
[null," "," "," "]
["  表4"," "," "," "]
["单位工程造价汇总表"]
["工程名称：三层会议室及办公室_安装单位工程",null,"第2页 共4页"]
["序号","汇  总  内  容",null,"金额（元）"]
[" "," ",null," "]
["1","分部分项工程费",null,"7131.16"]
["1.1","电气工程",null,"7131.16"]
["2","措施项目费",null,"221.71"]
["2.1","总价措施项目费",null,"94.62"]
["2.1.1","安全文明施工费",null,"69.46"]
["2.1.2","其他总价措施费",null,"7.98"]
["2.1.3","扬尘防治措施费",null,"8.47"]
["2.1.4","建筑工人实名制措施费",null,"8.71"]
["2.2","单价措施项目费",null,"127.09"]
["3","其他项目费",null,"0"]
["3.1","暂列金额",null,"0"]
["3.2","专业工程暂估价",null,"0"]
["3.3","总承包服务费",null,"0"]
["合计=1+2+3",null,null,"7352.87"]
[]
[null," "," "," "]
["  表4"," "," "," "]
["单位工程造价汇总表"]
["工程名称：六层会议室及办公室_土建单位工程",null,"第3页 共4页"]
["序号","汇  总  内  容",null,"金额（元）"]
[" "," ",null," "]
[" "," ",null," "]
["1","分部分项工程费",null,"24537.24"]
["1.1","土石方工程",null,"216.7"]
["1.2","砌筑工程",null,"173.97"]
["1.3","门窗工程",null,"5993.16"]
["1.4","墙、柱面装饰与隔断、幕墙工程",null,"118.12"]
["1.5","天棚工程",null,"12780.15"]
["1.6","油漆、涂料、裱糊工程",null,"4442.76"]
["1.7","拆除工程",null,"812.38"]
["2","措施项目费",null,"3297.66"]
["2.1","总价措施项目费",null,"358.22"]
["2.1.1","安全文明施工费",null,"262.95"]
["2.1.2","其他总价措施费",null,"30.22"]
["2.1.3","扬尘防治措施费",null,"32.08"]
["2.1.4","建筑工人实名制措施费",null,"32.97"]
["2.2","单价措施项目费",null,"2939.44"]
["3","其他项目费",null,"24"]
["3.1","暂列金额",null,"24"]
["3.2","专业工程暂估价",null,"0"]
["3.3","总承包服务费",null,"0"]
["合计=1+2+3",null,null,"27858.9"]
[]
[null," "," "," "]
["  表4"," "," "," "]
["单位工程造价汇总表"]
["工程名称：六层会议室及办公室_安装单位工程",null,"第4页 共4页"]
["序号","汇  总  内  容",null,"金额（元）"]
[" "," ",null," "]
["1","分部分项工程费",null,"9897.76"]
["1.1","电气工程",null,"9897.76"]
["2","措施项目费",null,"304.11"]
["2.1","总价措施项目费",null,"131.3"]
["2.1.1","安全文明施工费",null,"96.38"]
["2.1.2","其他总价措施费",null,"11.08"]
["2.1.3","扬尘防治措施费",null,"11.76"]
["2.1.4","建筑工人实名制措施费",null,"12.08"]
["2.2","单价措施项目费",null,"172.81"]
["3","其他项目费",null,"0"]
["3.1","暂列金额",null,"0"]
["3.2","专业工程暂估价",null,"0"]
["3.3","总承包服务费",null,"0"]
["合计=1+2+3",null,null,"10201.87"]
[]
[null," "," "," "]

{"sheet":"表05分部分项工程量清单与计价表","index":4,"n_rows":114,"n_cols":8,"rows_kept":114,"merged":[[0,0,0,1],[1,0,1,7],[2,0,2,5],[2,6,2,7],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,3,7],[7,1,7,7],[11,0,11,6],[12,1,12,7],[14,0,14,6],[15,1,15,7],[17,0,17,6],[18,1,18,7],[20,0,20,6],[21,0,21,6],[23,6,23,7],[24,0,24,1],[25,0,25,7],[26,0,26,5],[26,6,26,7],[27,0,28,0],[27,1,28,1],[27,2,28,2],[27,3,28,3],[27,4,28,4],[27,5,28,5],[27,6,27,7],[30,1,30,7],[41,0,41,6],[42,0,42,6],[44,6,44,7],[45,0,45,1],[46,0,46,7],[47,0,47,5],[47,6,47,7],[48,0,49,0],[48,1,49,1],[48,2,49,2],[48,3,49,3],[48,4,49,4],[48,5,49,5],[48,6,48,7],[52,1,52,7],[54,0,54,6],[55,1,55,7],[57,0,57,6],[58,1,58,7],[63,0,63,6],[64,1,64,7],[66,0,66,6],[67,1,67,7],[69,0,69,6],[70,1,70,7],[72,0,72,6],[74,6,74,7],[75,0,75,1],[76,0,76,7],[77,0,77,5],[77,6,77,7],[78,0,79,0],[78,1,79,1],[78,2,79,2],[78,3,79,3],[78,4,79,4],[78,5,79,5],[78,6,78,7],[80,1,80,7],[85,0,85,6],[86,0,86,6],[88,6,88,7],[89,0,89,1],[90,0,90,7],[91,0,91,5],[91,6,91,7],[92,0,93,0],[92,1,93,1],[92,2,93,2],[92,3,93,3],[92,4,93,4],[92,5,93,5],[92,6,92,7],[95,1,95,7],[110,0,110,6],[111,0,111,6],[113,6,113,7]],"flags":["formulas_cached_only"]}
["  表5",null," "," "," "," "," "," "]
["分部分项工程量清单与计价表"]
["工程名称：三层会议室及办公室_土建单位工程",{"$nulls":5},"第1页 共5页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量","金   额（元）"]
[{"$nulls":6},"综合\n单价","合  价"]
[" "," "," "," "," "," "," "," "]
[" "," "," "," "," "," "," "," "]
["一","门窗工程"]
["1","010802001001","金属（塑钢）门","  1.门代号及洞口尺寸:M15235 \n1500*2350\n  2.门框、扇材质:浅灰色塑钢\n双开门（具体颜色需同二层销售\n部门）","m2","3.53","505.04","1782.79"]
["2","010810004001","铝合金窗帘盒","  1.窗帘盒材质、规格:140宽铝\n合金","m","16","109.89","1758.24"]
["3","010810005001","窗帘轨","1.窗帘轨材质、规格:铝合金窗\n轨（单轨）","m","16","29.09","465.44"]
["小     计",{"$nulls":6},"4006.47"]
["二","天棚工程"]
["1","011302001001","天棚吊顶","  1.600*600mm3厚铝塑板吊顶\n  2.装配式U型轻钢（不上人型\n）","m2","87.52","144.67","12661.52"]
["小     计",{"$nulls":6},"12661.52"]
["三","油漆、涂料、裱糊工程"]
["1","011406001001","抹灰面油漆涂料","  1.翻新门后部分墙面面层","m2","3","31.09","93.27"]
["小     计",{"$nulls":6},"93.27"]
["四","拆除工程"]
["1","011610001001","门窗拆除","  1.拆除整樘钢门窗 2.5M2<每\n樘面积≦4M2","樘","1","50.91","50.91"]
["小     计",{"$nulls":6},"50.91"]
["合     计",{"$nulls":6},"16812.17"]
[]
[{"$nulls":4}," "," "," "]
["  表5",null," "," "," "," "," "," "]
["分部分项工程量清单与计价表"]
["工程名称：三层会议室及办公室_安装单位工程",{"$nulls":5},"第2页 共5页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量","金   额（元）"]
[{"$nulls":6},"综合\n单价","合  价"]
[" "," "," "," "," "," "," "," "]
["一","电气工程"]
["1","030901003001","水喷淋(雾)喷头","1.喷头DN25","个","9","32.14","289.26"]
["2","030901001001","水喷淋钢管","1.钢管螺纹连接 DN25","m","7","43.48","304.36"]
["3","030412005001","荧光灯","1.吊顶灯600*6000","套","9","262.48","2362.32"]
["4","030404035001","插座","1.五孔插座","个","10","18.76","187.6"]
["5","030404034001","照明开关","1.双联开关","个","4","19.58","78.32"]
["6","030411001001","配管","1.刚性阻燃管敷设 砖、混凝土\n结构暗配 PVC20","m","150","9.57","1435.5"]
["7","030411001002","配管","1.金属软管敷设 DN20 ( 每根长\n≤0.5m)","m","10","53.04","530.4"]
["8","030411004001","配线","1.管内穿线 穿照明线 铜芯 BV-\n2.5","m","420","3.66","1537.2"]
["9","030411004002","配线","1.管内穿线 穿照明线 铜芯 BV-\n4","m","60","4.27","256.2"]
["10","030901010001","室内消火栓","  1.更换消火栓箱门（\n650*800mm）","套","1","150","150"]
["小     计",{"$nulls":6},"7131.16"]
["合     计",{"$nulls":6},"7131.16"]
[]
[{"$nulls":4}," "," "," "]
["  表5",null," "," "," "," "," "," "]
["分部分项工程量清单与计价表"]
["工程名称：六层会议室及办公室_土建单位工程",{"$nulls":5},"第3页 共5页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量","金   额（元）"]
[{"$nulls":6},"综合\n单价","合  价"]
[" "," "," "," "," "," "," "," "]
[" "," "," "," "," "," "," "," "]
["一","土石方工程"]
["1","010103002001","余方弃置","  1.废弃料品种：拆除废弃物\n  2.运距:暂按10km，结算时据\n实调整","m3","7.54","28.74","216.7"]
["小     计",{"$nulls":6},"216.7"]
["二","砌筑工程"]
["1","010401012001","零星砌砖","1.零星砌砖名称、部位:洞口填\n堵\n2.砖品种、规格、强度等级:烧\n结煤矸石普通砖\n3.砂浆强度等级、配合比:混合\n砂浆M5","m3","0.19","915.63","173.97"]
["小     计",{"$nulls":6},"173.97"]
["三","门窗工程"]
["1","010802001002","金属（塑钢）门","  1.门代号及洞口尺寸:M15235 \n1500*2350\n  2.门框、扇材质:浅灰色塑钢\n双开门（具体颜色需同二层销售\n部门）","m2","3.53","505.04","1782.79"]
["2","010802001003","金属（塑钢）门","  1.门代号及洞口尺寸:M1024 \n1000*2400\n  2.门框、扇材质:浅灰色塑钢\n平开门（双层门）（具体颜色需\n同二层销售部门）","m2","2.4","932.02","2236.85"]
["3","010810004002","铝合金窗帘盒","  1.窗帘盒材质、规格:140宽铝\n合金","m","14.2","109.89","1560.44"]
["4","010810005002","窗帘轨","1.窗帘轨材质、规格:铝合金窗\n轨（单轨）","m","14.2","29.09","413.08"]
["小     计",{"$nulls":6},"5993.16"]
["四","墙、柱面装饰与隔断、幕墙工程"]
["1","011203003001","零星项目砂浆找平","  填堵窗户处找平\n  1.找平的砂浆厚度、配合比\n:5厚1：2.5水泥砂浆，9厚1:3水\n泥砂浆","m2","1.9","62.17","118.12"]
["小     计",{"$nulls":6},"118.12"]
["五","天棚工程"]
["1","011302001002","天棚吊顶","  1.600*600mm3厚铝塑板吊顶\n  2.装配式U型轻钢（不上人型\n）","m2","88.34","144.67","12780.15"]
["小     计",{"$nulls":6},"12780.15"]
["六","油漆、涂料、裱糊工程"]
["1","011406001002","抹灰面油漆涂料","  1.腻子种类、遍数:满刮腻子\n二遍\n  2.油漆涂料品种、遍数（或厚\n度）:乳液型涂料二遍","m2","142.9","31.09","4442.76"]
["小     计",{"$nulls":6},"4442.76"]
[]
[{"$nulls":4}," "," "," "]
["  表5",null," "," "," "," "," "," "]
["分部分项工程量清单与计价表"]
["工程名称：六层会议室及办公室_土建单位工程",{"$nulls":5},"第4页 共5页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量","金   额（元）"]
[{"$nulls":6},"综合\n单价","合  价"]
["七","拆除工程"]
["1","011610001002","门窗拆除","  1.拆除整樘门窗","樘","1","26.13","26.13"]
["2","011610001003","门窗拆除","  1.拆除整樘门窗 双层门窗","樘","1","36.56","36.56"]
["3","011610001004","门窗拆除","  1.拆除整樘钢门窗 2.5M2<每\n樘面积≦4M2","樘","1","50.91","50.91"]
["4","011608001001","铲除油漆涂料面","  1.清除抹灰面油漆涂料","m2","142.9","4.89","698.78"]
["小     计",{"$nulls":6},"812.38"]
["合     计",{"$nulls":6},"24537.24"]
[]
[{"$nulls":4}," "," "," "]
["  表5",null," "," "," "," "," "," "]
["分部分项工程量清单与计价表"]
["工程名称：六层会议室及办公室_安装单位工程",{"$nulls":5},"第5页 共5页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量","金   额（元）"]
[{"$nulls":6},"综合\n单价","合  价"]
[" "," "," "," "," "," "," "," "]
["一","电气工程"]
["1","030901003002","水喷淋(雾)喷头","1.喷头DN25","个","9","32.14","289.26"]
["2","030901001002","水喷淋钢管","1.钢管螺纹连接 DN25","m","7","43.48","304.36"]
["3","030412005002","荧光灯","1.吊顶灯600*6000","套","9","262.48","2362.32"]
["4","030404035002","插座","1.五孔插座","个","20","18.76","375.2"]
["5","030404034002","照明开关","1.双联开关","个","4","19.58","78.32"]
["6","030404035003","插座","1.空调插座","个","4","29.9","119.6"]
["7","030411001003","配管","1.刚性阻燃管敷设 砖、混凝土\n结构暗配 PVC20","m","200","9.57","1914"]
["8","030411001004","配管","1.金属软管敷设 DN20 ( 每根长\n≤0.5m)","m","10","53.04","530.4"]
["9","030411004003","配线","1.管内穿线 穿照明线 铜芯 BV-\n2.5","m","590","3.66","2159.4"]
["10","030411004004","配线","1.管内穿线 穿照明线 铜芯 BV-\n4","m","40","4.27","170.8"]
["11","030901010002","室内消火栓","1.更换消火栓箱门（\n650*800mm）","套","1","150","150"]
["12","BC01001","消防管改接","  1.消防管改接","项","1","800","800"]
["13","030413002001","凿(压)槽","  1.剔堵槽、沟 砖结构 宽\nmm*深mm (70*70)","m","20","24.7","494"]
["14","030411002001","线槽","1.塑料线槽敷设 DN25","m","10","15.01","150.1"]
["小     计",{"$nulls":6},"9897.76"]
["合     计",{"$nulls":6},"9897.76"]
[]
[{"$nulls":4}," "," "," "]

{"sheet":"表06总价措施项目清单与计价表","index":5,"n_rows":50,"n_cols":5,"rows_kept":50,"merged":[[1,0,1,4],[2,0,2,2],[2,3,2,4],[10,0,10,3],[14,0,14,4],[15,0,15,2],[15,3,15,4],[22,0,22,3],[26,0,26,4],[27,0,27,2],[27,3,27,4],[35,0,35,3],[39,0,39,4],[40,0,40,2],[40,3,40,4],[47,0,47,3]],"flags":["formulas_cached_only"]}
["  表6"," "," "," "," "]
["总价措施项目清单与计价表"]
["工程名称：三层会议室及办公室_土建单位工程",null,null,"第1页 共4页"]
["序号","项  目  名  称","计 算 基 础","费率（%）","金额（元）"]
[" "," "," "," "," "]
[" "," "," "," "," "]
["1","安全文明施工费","17554.54","0.957%","168"]
["2","其他总价措施费","17554.54","0.11%","19.31"]
["3","扬尘防治措施费","168","12.2%","20.5"]
["4","建筑工人实名制措施费","17554.54","0.12%","21.07"]
["合    计",{"$nulls":3},"228.88"]
[]
[null," "," "," "," "]
["  表6"," "," "," "," "]
["总价措施项目清单与计价表"]
["工程名称：三层会议室及办公室_安装单位工程",null,null,"第2页 共4页"]
["序号","项  目  名  称","计 算 基 础","费率（%）","金额（元）"]
[" "," "," "," "," "]
["1","安全文明施工费","7258.25","0.957%","69.46"]
["2","其他总价措施费","7258.25","0.11%","7.98"]
["3","扬尘防治措施费","69.46","12.2%","8.47"]
["4","建筑工人实名制措施费","7258.25","0.12%","8.71"]
["合    计",{"$nulls":3},"94.62"]
[]
[null," "," "," "," "]
["  表6"," "," "," "," "]
["总价措施项目清单与计价表"]
["工程名称：六层会议室及办公室_土建单位工程",null,null,"第3页 共4页"]
["序号","项  目  名  称","计 算 基 础","费率（%）","金额（元）"]
[" "," "," "," "," "]
[" "," "," "," "," "]
["1","安全文明施工费","27476.68","0.957%","262.95"]
["2","其他总价措施费","27476.68","0.11%","30.22"]
["3","扬尘防治措施费","262.95","12.2%","32.08"]
["4","建筑工人实名制措施费","27476.68","0.12%","32.97"]
["合    计",{"$nulls":3},"358.22"]
[]
[null," "," "," "," "]
["  表6"," "," "," "," "]
["总价措施项目清单与计价表"]
["工程名称：六层会议室及办公室_安装单位工程",null,null,"第4页 共4页"]
["序号","项  目  名  称","计 算 基 础","费率（%）","金额（元）"]
[" "," "," "," "," "]
["1","安全文明施工费","10070.57","0.957%","96.38"]
["2","其他总价措施费","10070.57","0.11%","11.08"]
["3","扬尘防治措施费","96.38","12.2%","11.76"]
["4","建筑工人实名制措施费","10070.57","0.12%","12.08"]
["合    计",{"$nulls":3},"131.3"]
[]
[null," "," "," "," "]

{"sheet":"表07单价措施项目清单与计价表","index":6,"n_rows":70,"n_cols":8,"rows_kept":70,"merged":[[1,0,1,7],[2,0,2,6],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,3,7],[7,1,7,7],[12,0,12,6],[13,0,13,6],[15,6,15,7],[17,0,17,7],[18,0,18,6],[19,0,20,0],[19,1,20,1],[19,2,20,2],[19,3,20,3],[19,4,20,4],[19,5,20,5],[19,6,19,7],[22,1,22,7],[23,1,23,7],[27,0,27,6],[28,0,28,6],[30,6,30,7],[32,0,32,7],[33,0,33,6],[34,0,35,0],[34,1,35,1],[34,2,35,2],[34,3,35,3],[34,4,35,4],[34,5,35,5],[34,6,34,7],[38,1,38,7],[41,0,41,6],[42,1,42,7],[50,0,50,6],[51,0,51,6],[53,6,53,7],[55,0,55,7],[56,0,56,6],[57,0,58,0],[57,1,58,1],[57,2,58,2],[57,3,58,3],[57,4,58,4],[57,5,58,5],[57,6,57,7],[60,1,60,7],[61,1,61,7],[66,0,66,6],[67,0,67,6],[69,6,69,7]],"flags":["formulas_cached_only"]}
["  表7"," "," "," "," "," "," "," "]
["单价措施项目清单与计价表"]
["工程名称：三层会议室及办公室_土建单位工程",{"$nulls":6},"第1页 共4页"]
["序号","项目编码","项目名称","项目特征描述","计量单位","工程量","金     额（元）"]
[{"$nulls":6},"综合单价","合价"]
[" "," "," "," "," "," "," "," "]
[" "," "," "," "," "," "," "," "]
["一","其他措施项目"]
["1","011703001001","垂直运输","  1.人工搬运 \n( 各种胶合板材\n、石膏板 每上\n2层楼)\n  2.人工搬运 \n( 门窗 每上2层\n楼)\n  3.人工搬运 \n( 钢筋、水泥、\n石灰、油漆、涂\n料  每上2层楼)","项","1","742.37","742.37"]
["(1)","10117107换1","人工搬运 ( 各\n种胶合板材、石\n膏板 每上2层楼\n)"," ","m2","192.54","3.78","727.8"]
["(2)","10117110换1","人工搬运 ( 门\n窗 每上2层楼)"," ","m2","3.39","1.53","5.19"]
["(3)","10117104换1","人工搬运 ( 钢\n筋、水泥、石灰\n、油漆、涂料  \n每上2层楼)"," ","t","0.066","142.17","9.38"]
["小     计",{"$nulls":6},"742.37"]
["合     计",{"$nulls":6},"742.37"]
[]
[{"$nulls":3}," "," "," "," "]
["  表7"," "," "," "," "," "," "," "]
["单价措施项目清单与计价表"]
["工程名称：三层会议室及办公室_安装单位工程",{"$nulls":6},"第2页 共4页"]
["序号","项目编码","项目名称","项目特征描述","计量单位","工程量","金     额（元）"]
[{"$nulls":6},"综合单价","合价"]
[" "," "," "," "," "," "," "," "]
["一","措施分部L01"]
["二","措施项目"]
["1","031301017001","脚手架搭拆"," ","项","1","127.09","127.09"]
["(1)","JSJ009","消防脚手架搭拆\n费"," ","元","12.378","1.28","15.84"]
["(2)","JSJ005","电气设备安装脚\n手架搭拆费"," ","元","86.915","1.28","111.25"]
["小     计",{"$nulls":6},"127.09"]
["合     计",{"$nulls":6},"127.09"]
[]
[{"$nulls":3}," "," "," "," "]
["  表7"," "," "," "," "," "," "," "]
["单价措施项目清单与计价表"]
["工程名称：六层会议室及办公室_土建单位工程",{"$nulls":6},"第3页 共4页"]
["序号","项目编码","项目名称","项目特征描述","计量单位","工程量","金     额（元）"]
[{"$nulls":6},"综合单价","合价"]
[" "," "," "," "," "," "," "," "]
[" "," "," "," "," "," "," "," "]
["一","脚手架"]
["1","011701003001","砌筑脚手架","1.里脚手架","m2","4.47","3.8","16.99"]
["(1)","10117017","里脚手架"," ","m2","4.47","3.8","16.99"]
["小     计",{"$nulls":6},"16.99"]
["二","其他措施项目"]
["1","011703001002","垂直运输","  1.人工搬运 \n( 砖、砌块、碎\n石、砂土  每上\n五层楼)\n  2.人工搬运 \n( 钢筋、水泥、\n石灰、油漆、涂\n料  每上五层楼\n)\n  3.人工搬运 \n( 各种胶合板材\n、石膏板 每上\n五层楼)\n  4.人工搬运 \n( 门窗 每上五\n层楼)","项","1","1622.48","1622.48"]
["(1)","10117103换1","人工搬运 ( 砖\n、砌块、碎石、\n砂土  每上五层\n楼)"," ","m3","0.14","121.55","17.02"]
["(2)","10117104换2","人工搬运 ( 钢\n筋、水泥、石灰\n、油漆、涂料  \n每上五层楼)"," ","t","0.425","284.36","120.85"]
["(3)","10117107换2","人工搬运 ( 各\n种胶合板材、石\n膏板 每上五层\n楼)"," ","m2","194.35","7.55","1467.34"]
["(4)","10117110换2","人工搬运 ( 门\n窗 每上五层楼)"," ","m2","5.7","3.03","17.27"]
["2","011703001003","垂直运输","1.人工搬运 ( \n垃圾每向下5层\n楼)","项","1","1299.97","1299.97"]
["(1)","10117113换1","人工搬运 ( 垃\n圾每向下5层楼)"," ","m3","7.54","172.41","1299.97"]
["小     计",{"$nulls":6},"2922.45"]
["合     计",{"$nulls":6},"2939.44"]
[]
[{"$nulls":3}," "," "," "," "]
["  表7"," "," "," "," "," "," "," "]
["单价措施项目清单与计价表"]
["工程名称：六层会议室及办公室_安装单位工程",{"$nulls":6},"第4页 共4页"]
["序号","项目编码","项目名称","项目特征描述","计量单位","工程量","金     额（元）"]
[{"$nulls":6},"综合单价","合价"]
[" "," "," "," "," "," "," "," "]
["一","措施分部L01"]
["二","措施项目"]
["1","031301017002","脚手架搭拆"," ","项","1","172.81","172.81"]
["(1)","JSJ009","消防脚手架搭拆\n费"," ","元","12.378","1.28","15.84"]
["(2)","JSJ005","电气设备安装脚\n手架搭拆费"," ","元","113.859","1.28","145.74"]
["(3)","JSJ010","给排水、采暖、\n燃气脚手架搭拆\n费"," ","元","8.77","1.28","11.23"]
["小     计",{"$nulls":6},"172.81"]
["合     计",{"$nulls":6},"172.81"]
[]
[{"$nulls":3}," "," "," "," "]

{"sheet":"表10分部分项工程量清单综合单价分析表","index":7,"n_rows":169,"n_cols":14,"rows_kept":169,"merged":[[0,0,0,1],[1,0,1,13],[2,0,2,10],[2,11,2,13],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,3,12],[3,13,4,13],[7,1,7,13],[14,1,14,13],[18,1,18,13],[22,0,22,1],[23,0,23,13],[24,0,24,10],[24,11,24,13],[25,0,26,0],[25,1,26,1],[25,2,26,2],[25,3,26,3],[25,4,26,4],[25,5,25,12],[25,13,26,13],[28,1,28,13],[33,0,33,1],[34,0,34,13],[35,0,35,10],[35,11,35,13],[36,0,37,0],[36,1,37,1],[36,2,37,2],[36,3,37,3],[36,4,37,4],[36,5,36,12],[36,13,37,13],[39,1,39,13],[56,0,56,1],[57,0,57,13],[58,0,58,10],[58,11,58,13],[59,0,60,0],[59,1,60,1],[59,2,60,2],[59,3,60,3],[59,4,60,4],[59,5,59,12],[59,13,60,13],[69,0,69,1],[70,0,70,13],[71,0,71,10],[71,11,71,13],[72,0,73,0],[72,1,73,1],[72,2,73,2],[72,3,73,3],[72,4,73,4],[72,5,72,12],[72,13,73,13],[76,1,76,13],[79,1,79,13],[82,1,82,13],[87,0,87,1],[88,0,88,13],[89,0,89,10],[89,11,89,13],[90,0,91,0],[90,1,91,1],[90,2,91,2],[90,3,91,3],[90,4,91,4],[90,5,90,12],[90,13,91,13],[98,1,98,13],[101,1,101,13],[105,0,105,1],[106,0,106,13],[107,0,107,10],[107,11,107,13],[108,0,109,0],[108,1,109,1],[108,2,109,2],[108,3,109,3],[108,4,109,4],[108,5,108,12],[108,13,109,13],[111,1,111,13],[114,1,114,13],[125,0,125,1],[126,0,126,13],[127,0,127,10],[127,11,127,13],[128,0,129,0],[128,1,129,1],[128,2,129,2],[128,3,129,3],[128,4,129,4],[128,5,128,12],[128,13,129,13],[131,1,131,13],[148,0,148,1],[149,0,149,13],[150,0,150,10],[150,11,150,13],[151,0,152,0],[151,1,152,1],[151,2,152,2],[151,3,152,3],[151,4,152,4],[151,5,151,12],[151,13,152,13]],"flags":["formulas_cached_only"]}
["  表10",null," "," "," "," "," "," "," "," "," "," "," "," "]
["分部分项工程量清单综合单价分析表"]
["工程名称：三层会议室及办公室_土建单位工程",{"$nulls":10},"第1页 共9页"]
["序号","项目编码","项目名称及特征描述","单位","工程量","综合单价组成（元）",{"$nulls":7},"综合单价\n（元）"]
[{"$nulls":5},"人工费","材料费","其中：\n设备费","施工机具使用费","企业管理费","利润","规费","税金"]
[" "," "," "," "," "," "," "," "," "," "," "," "," "," "]
[" "," "," "," "," "," "," "," "," "," "," "," "," "," "]
["一","门窗工程"]
["1","010802001001","金属（塑钢）门\n  1.门代号及洞口尺寸:M15235 \n1500*2350\n  2.门框、扇材质:浅灰色塑钢双开\n门（具体颜色需同二层销售部门）","m2","3.53","43.29","355.37","0.00","0.00","39.07","26.27","0.00","41.76","505.04"]
["1.1","10108023换1","塑钢双开门","m2","3.53","43.23","354.87","0.00","0.00","39.01","26.23","0.00","41.70","505.04"]
["2","010810004001","铝合金窗帘盒\n  1.窗帘盒材质、规格:140宽铝合\n金","m","16","20.33","66.29","0.00","0.00","8.49","5.71","0.00","9.07","109.89"]
["2.1","10108100","铝合金窗帘盒","m","16","20.33","66.29","0.00","0.00","8.49","5.71","0.00","9.07","109.89"]
["3","010810005001","窗帘轨\n1.窗帘轨材质、规格:铝合金窗轨（\n单轨）","m","16","4.57","18.36","0.00","0.00","2.25","1.51","0.00","2.40","29.09"]
["3.1","10108101","暗装 (单轨)","m","16","4.57","18.36","0.00","0.00","2.25","1.51","0.00","2.40","29.09"]
["二","天棚工程"]
["1","011302001001","天棚吊顶\n  1.600*600mm3厚铝塑板吊顶\n  2.装配式U型轻钢（不上人型）","m2","87.52","42.36","69.37","0.00","2.30","11.18","7.51","0.00","11.95","144.67"]
["1.1","10113019","装配式U型轻钢（不上人型） (面层\n规格(600mm×600mm)  平面)","m2","87.52","20.12","31.23","0.00","2.30","5.26","3.53","0.00","5.62","68.06"]
["1.2","10113081","铝塑板天棚面层 (贴在龙骨底)","m2","87.52","22.24","38.14","0.00","0.00","5.92","3.98","0.00","6.33","76.61"]
["三","油漆、涂料、裱糊工程"]
["1","011406001001","抹灰面油漆涂料\n  1.翻新门后部分墙面面层","m2","3","16.04","8.47","0.00","0.00","2.40","1.61","0.00","2.57","31.09"]
[]
[null,null," "," "," "," "," "," "," "," "," "," "," "," "]
["  表10",null," "," "," "," "," "," "," "," "," "," "," "," "]
["分部分项工程量清单综合单价分析表"]
["工程名称：三层会议室及办公室_土建单位工程",{"$nulls":10},"第2页 共9页"]
["序号","项目编码","项目名称及特征描述","单位","工程量","综合单价组成（元）",{"$nulls":7},"综合单价\n（元）"]
[{"$nulls":5},"人工费","材料费","其中：\n设备费","施工机具使用费","企业管理费","利润","规费","税金"]
["1.1","10114147","内墙涂料 (墙面 二遍)","m2","3","16.04","8.47","0.00","0.00","2.40","1.61","0.00","2.57","31.09"]
["四","拆除工程"]
["1","011610001001","门窗拆除\n  1.拆除整樘钢门窗 2.5M2<每樘面\n积≦4M2","樘","1","40.14","0.00","0.00","0.00","3.93","2.64","0.00","4.20","50.91"]
["1.1","10116103换1","拆除整樘钢门窗 2.5M2<每樘面积≦\n4M2","樘","1","40.14","0.00","0.00","0.00","3.93","2.64","0.00","4.20","50.91"]
[]
[null,null," "," "," "," "," "," "," "," "," "," "," "," "]
["  表10",null," "," "," "," "," "," "," "," "," "," "," "," "]
["分部分项工程量清单综合单价分析表"]
["工程名称：三层会议室及办公室_安装单位工程",{"$nulls":10},"第3页 共9页"]
["序号","项目编码","项目名称及特征描述","单位","工程量","综合单价组成（元）",{"$nulls":7},"综合单价\n（元）"]
[{"$nulls":5},"人工费","材料费","其中：\n设备费","施工机具使用费","企业管理费","利润","规费","税金"]
[" "," "," "," "," "," "," "," "," "," "," "," "," "," "]
["一","电气工程"]
["1","030901003001","水喷淋(雾)喷头\n1.喷头DN25","个","9","11.95","13.25","0.00","0.14","2.48","1.67","0.00","2.65","32.14"]
["1.1","30901036换1","喷头DN25","个","9","11.95","13.25","0.00","0.14","2.48","1.67","0.00","2.65","32.14"]
["2","030901001001","水喷淋钢管\n1.钢管螺纹连接 DN25","m","7","20.00","14.00","0.00","0.27","3.36","2.26","0.00","3.59","43.48"]
["2.1","30901001换1","钢管螺纹连接 DN25","m","7","20.00","14.00","0.00","0.27","3.36","2.26","0.00","3.59","43.48"]
["3","030412005001","荧光灯\n1.吊顶灯600*6000","套","9","9.86","197.04","0.00","0.00","20.28","13.63","0.00","21.67","262.48"]
["3.1","30414004换1","吊顶灯600*6000","套","9","9.86","197.04","0.00","0.00","20.28","13.63","0.00","21.67","262.48"]
["4","030404035001","插座\n1.五孔插座","个","10","6.25","8.54","0.00","0.00","1.45","0.97","0.00","1.55","18.76"]
["4.1","30414305换1","五孔插座","套","10","6.25","8.54","0.00","0.00","1.45","0.97","0.00","1.55","18.76"]
["5","030404034001","照明开关\n1.双联开关","个","4","6.25","9.18","0.00","0.00","1.51","1.02","0.00","1.62","19.58"]
["5.1","30414284换1","双联开关","套","4","6.25","9.18","0.00","0.00","1.51","1.02","0.00","1.62","19.58"]
["6","030411001001","配管\n1.刚性阻燃管敷设 砖、混凝土结构\n暗配 PVC20","m","150","6.22","1.32","0.00","0.00","0.74","0.50","0.00","0.79","9.57"]
["6.1","30412187换1","刚性阻燃管敷设 砖、混凝土结构暗\n配 PVC20","m","150","6.22","1.32","0.00","0.00","0.74","0.50","0.00","0.79","9.57"]
["7","030411001002","配管\n1.金属软管敷设 DN20 ( 每根长≤\n0.5m)","m","10","30.86","10.95","0.00","0.00","4.10","2.75","0.00","4.38","53.04"]
["7.1","30412227换1","金属软管敷设 DN20 ( 每根长≤\n0.5m)","m","10","30.86","10.95","0.00","0.00","4.10","2.75","0.00","4.38","53.04"]
[]
[null,null," "," "," "," "," "," "," "," "," "," "," "," "]
["  表10",null," "," "," "," "," "," "," "," "," "," "," "," "]
["分部分项工程量清单综合单价分析表"]
["工程名称：三层会议室及办公室_安装单位工程",{"$nulls":10},"第4页 共9页"]
["序号","项目编码","项目名称及特征描述","单位","工程量","综合单价组成（元）",{"$nulls":7},"综合单价\n（元）"]
[{"$nulls":5},"人工费","材料费","其中：\n设备费","施工机具使用费","企业管理费","利润","规费","税金"]
["8","030411004001","配线\n1.管内穿线 穿照明线 铜芯 BV-2.5","m","420","0.89","2.00","0.00","0.00","0.28","0.19","0.00","0.30","3.66"]
["8.1","30413005换1","管内穿线 穿照明线 铜芯 BV-2.5","单线","420","0.89","2.00","0.00","0.00","0.28","0.19","0.00","0.30","3.66"]
["9","030411004002","配线\n1.管内穿线 穿照明线 铜芯 BV-4","m","60","0.59","2.78","0.00","0.00","0.33","0.22","0.00","0.35","4.27"]
["9.1","30413006换1","管内穿线 穿照明线 铜芯 BV-4","单线","60","0.59","2.78","0.00","0.00","0.33","0.22","0.00","0.35","4.27"]
["10","030901010001","室内消火栓\n  1.更换消火栓箱门（650*800mm）","套","1","0.00","0.00","0.00","0.00","0.00","0.00","0.00","0.00","150"]
["10.1","bc0101","更换消火栓箱门（650*800mm）","套","1","0.00","0.00","0.00","0.00","0.00","0.00","0.00","0.00","150"]
[]
[null,null," "," "," "," "," "," "," "," "," "," "," "," "]
["  表10",null," "," "," "," "," "," "," "," "," "," "," "," "]
["分部分项工程量清单综合单价分析表"]
["工程名称：六层会议室及办公室_土建单位工程",{"$nulls":10},"第5页 共9页"]
["序号","项目编码","项目名称及特征描述","单位","工程量","综合单价组成（元）",{"$nulls":7},"综合单价\n（元）"]
[{"$nulls":5},"人工费","材料费","其中：\n设备费","施工机具使用费","企业管理费","利润","规费","税金"]
[" "," "," "," "," "," "," "," "," "," "," "," "," "," "]
[" "," "," "," "," "," "," "," "," "," "," "," "," "," "]
["一","土石方工程"]
["1","010103002001","余方弃置\n  1.废弃料品种：拆除废弃物\n  2.运距:暂按10km，结算时据实调\n整","m3","7.54","0.16","0.00","0.00","22.50","2.22","1.49","0.00","2.37","28.74"]
["1.1","10101084换1","自卸汽车运土 (载重10t以内运距\n10km)","m3","7.54","0.16","0.00","0.00","22.50","2.22","1.49","0.00","2.37","28.74"]
["二","砌筑工程"]
["1","010401012001","零星砌砖\n1.零星砌砖名称、部位:洞口填堵\n2.砖品种、规格、强度等级:烧结煤\n矸石普通砖\n3.砂浆强度等级、配合比:混合砂浆\nM5","m3","0.19","365.49","352.32","0.00","3.96","70.73","47.55","0.00","75.60","915.63"]
["1.1","10104012","零星砖砌体","m3","0.19","365.49","352.32","0.00","3.96","70.73","47.55","0.00","75.60","915.65"]
["三","门窗工程"]
["1","010802001002","金属（塑钢）门\n  1.门代号及洞口尺寸:M15235 \n1500*2350\n  2.门框、扇材质:浅灰色塑钢双开\n门（具体颜色需同二层销售部门）","m2","3.53","43.29","355.37","0.00","0.00","39.07","26.27","0.00","41.76","505.04"]
["1.1","10108023换1","塑钢双开门","m2","3.53","43.23","354.87","0.00","0.00","39.01","26.23","0.00","41.70","505.04"]
[]
[null,null," "," "," "," "," "," "," "," "," "," "," "," "]
["  表10",null," "," "," "," "," "," "," "," "," "," "," "," "]
["分部分项工程量清单综合单价分析表"]
["工程名称：六层会议室及办公室_土建单位工程",{"$nulls":10},"第6页 共9页"]
["序号","项目编码","项目名称及特征描述","单位","工程量","综合单价组成（元）",{"$nulls":7},"综合单价\n（元）"]
[{"$nulls":5},"人工费","材料费","其中：\n设备费","施工机具使用费","企业管理费","利润","规费","税金"]
["2","010802001003","金属（塑钢）门\n  1.门代号及洞口尺寸:M1024 \n1000*2400\n  2.门框、扇材质:浅灰色塑钢平开\n门（双层门）（具体颜色需同二层\n销售部门）","m2","2.4","43.23","691.43","0.00","0.00","72.00","48.40","0.00","76.96","932.02"]
["2.1","10108023换3","塑钢平开门","m2","2.4","43.23","691.43","0.00","0.00","72.00","48.40","0.00","76.96","932.02"]
["3","010810004002","铝合金窗帘盒\n  1.窗帘盒材质、规格:140宽铝合\n金","m","14.2","20.33","66.29","0.00","0.00","8.49","5.71","0.00","9.07","109.89"]
["3.1","10108100","铝合金窗帘盒","m","14.2","20.33","66.29","0.00","0.00","8.49","5.71","0.00","9.07","109.89"]
["4","010810005002","窗帘轨\n1.窗帘轨材质、规格:铝合金窗轨（\n单轨）","m","14.2","4.57","18.36","0.00","0.00","2.25","1.51","0.00","2.40","29.09"]
["4.1","10108101","暗装 (单轨)","m","14.2","4.57","18.36","0.00","0.00","2.25","1.51","0.00","2.40","29.09"]
["四","墙、柱面装饰与隔断、幕墙工程"]
["1","011203003001","零星项目砂浆找平\n  填堵窗户处找平\n  1.找平的砂浆厚度、配合比:5厚\n1：2.5水泥砂浆，9厚1:3水泥砂浆","m2","1.9","44.54","4.13","0.00","0.34","4.80","3.23","0.00","5.13","62.17"]
["1.1","10112056","零星水泥砂浆找平抹灰（9+5mm厚）","m2","1.9","44.54","4.13","0.00","0.34","4.80","3.23","0.00","5.13","62.17"]
["五","天棚工程"]
["1","011302001002","天棚吊顶\n  1.600*600mm3厚铝塑板吊顶\n  2.装配式U型轻钢（不上人型）","m2","88.34","42.36","69.37","0.00","2.30","11.18","7.51","0.00","11.95","144.67"]
["1.1","10113019","装配式U型轻钢（不上人型） (面层\n规格(600mm×600mm)  平面)","m2","88.34","20.12","31.23","0.00","2.30","5.26","3.53","0.00","5.62","68.06"]
[null,null," "," "," "," "," "," "," "," "," "," "," "," "]
["  表10",null," "," "," "," "," "," "," "," "," "," "," "," "]
["分部分项工程量清单综合单价分析表"]
["工程名称：六层会议室及办公室_土建单位工程",{"$nulls":10},"第7页 共9页"]
["序号","项目编码","项目名称及特征描述","单位","工程量","综合单价组成（元）",{"$nulls":7},"综合单价\n（元）"]
[{"$nulls":5},"人工费","材料费","其中：\n设备费","施工机具使用费","企业管理费","利润","规费","税金"]
["1.2","10113081","铝塑板天棚面层 (贴在龙骨底)","m2","88.34","22.24","38.14","0.00","0.00","5.92","3.98","0.00","6.33","76.61"]
["六","油漆、涂料、裱糊工程"]
["1","011406001002","抹灰面油漆涂料\n  1.腻子种类、遍数:满刮腻子二遍\n  2.油漆涂料品种、遍数（或厚度\n）:乳液型涂料二遍","m2","142.9","16.04","8.47","0.00","0.00","2.40","1.61","0.00","2.57","31.09"]
["1.1","10114147","内墙涂料 (墙面 二遍)","m2","142.9","16.04","8.47","0.00","0.00","2.40","1.61","0.00","2.57","31.09"]
["七","拆除工程"]
["1","011610001002","门窗拆除\n  1.拆除整樘门窗","樘","1","20.59","0.00","0.00","0.00","2.02","1.36","0.00","2.16","26.13"]
["1.1","10116102","拆除整樘门窗","樘","1","20.59","0.00","0.00","0.00","2.02","1.36","0.00","2.16","26.13"]
["2","011610001003","门窗拆除\n  1.拆除整樘门窗 双层门窗","樘","1","28.82","0.00","0.00","0.00","2.82","1.90","0.00","3.02","36.56"]
["2.1","10116102换1","拆除整樘门窗 双层门窗","樘","1","28.82","0.00","0.00","0.00","2.82","1.90","0.00","3.02","36.56"]
["3","011610001004","门窗拆除\n  1.拆除整樘钢门窗 2.5M2<每樘面\n积≦4M2","樘","1","40.14","0.00","0.00","0.00","3.93","2.64","0.00","4.20","50.91"]
["3.1","10116103换2","拆除整樘钢门窗 2.5M2<每樘面积≦\n4M2","樘","1","40.14","0.00","0.00","0.00","3.93","2.64","0.00","4.20","50.91"]
["4","011608001001","铲除油漆涂料面\n  1.清除抹灰面油漆涂料","m2","142.9","3.86","0.00","0.00","0.00","0.38","0.25","0.00","0.40","4.89"]
["4.1","10116083","清除抹灰面油漆涂料","m2","142.9","3.86","0.00","0.00","0.00","0.38","0.25","0.00","0.40","4.89"]
[]
[null,null," "," "," "," "," "," "," "," "," "," "," "," "]
["  表10",null," "," "," "," "," "," "," "," "," "," "," "," "]
["分部分项工程量清单综合单价分析表"]
["工程名称：六层会议室及办公室_安装单位工程",{"$nulls":10},"第8页 共9页"]
["序号","项目编码","项目名称及特征描述","单位","工程量","综合单价组成（元）",{"$nulls":7},"综合单价\n（元）"]
[{"$nulls":5},"人工费","材料费","其中：\n设备费","施工机具使用费","企业管理费","利润","规费","税金"]
[" "," "," "," "," "," "," "," "," "," "," "," "," "," "]
["一","电气工程"]
["1","030901003002","水喷淋(雾)喷头\n1.喷头DN25","个","9","11.95","13.25","0.00","0.14","2.48","1.67","0.00","2.65","32.14"]
["1.1","30901036换1","喷头DN25","个","9","11.95","13.25","0.00","0.14","2.48","1.67","0.00","2.65","32.14"]
["2","030901001002","水喷淋钢管\n1.钢管螺纹连接 DN25","m","7","20.00","14.00","0.00","0.27","3.36","2.26","0.00","3.59","43.48"]
["2.1","30901001换1","钢管螺纹连接 DN25","m","7","20.00","14.00","0.00","0.27","3.36","2.26","0.00","3.59","43.48"]
["3","030412005002","荧光灯\n1.吊顶灯600*6000","套","9","9.86","197.04","0.00","0.00","20.28","13.63","0.00","21.67","262.48"]
["3.1","30414004换1","吊顶灯600*6000","套","9","9.86","197.04","0.00","0.00","20.28","13.63","0.00","21.67","262.48"]
["4","030404035002","插座\n1.五孔插座","个","20","6.25","8.54","0.00","0.00","1.45","0.97","0.00","1.55","18.76"]
["4.1","30414305换1","五孔插座","套","20","6.25","8.54","0.00","0.00","1.45","0.97","0.00","1.55","18.76"]
["5","030404034002","照明开关\n1.双联开关","个","4","6.25","9.18","0.00","0.00","1.51","1.02","0.00","1.62","19.58"]
["5.1","30414284换1","双联开关","套","4","6.25","9.18","0.00","0.00","1.51","1.02","0.00","1.62","19.58"]
["6","030404035003","插座\n1.空调插座","个","4","6.47","17.10","0.00","0.00","2.31","1.55","0.00","2.47","29.9"]
["6.1","30414306换1","空调插座","套","4","6.47","17.10","0.00","0.00","2.31","1.55","0.00","2.47","29.9"]
["7","030411001003","配管\n1.刚性阻燃管敷设 砖、混凝土结构\n暗配 PVC20","m","200","6.22","1.32","0.00","0.00","0.74","0.50","0.00","0.79","9.57"]
["7.1","30412187换1","刚性阻燃管敷设 砖、混凝土结构暗\n配 PVC20","m","200","6.22","1.32","0.00","0.00","0.74","0.50","0.00","0.79","9.57"]
[]
[null,null," "," "," "," "," "," "," "," "," "," "," "," "]
["  表10",null," "," "," "," "," "," "," "," "," "," "," "," "]
["分部分项工程量清单综合单价分析表"]
["工程名称：六层会议室及办公室_安装单位工程",{"$nulls":10},"第9页 共9页"]
["序号","项目编码","项目名称及特征描述","单位","工程量","综合单价组成（元）",{"$nulls":7},"综合单价\n（元）"]
[{"$nulls":5},"人工费","材料费","其中：\n设备费","施工机具使用费","企业管理费","利润","规费","税金"]
["8","030411001004","配管\n1.金属软管敷设 DN20 ( 每根长≤\n0.5m)","m","10","30.86","10.95","0.00","0.00","4.10","2.75","0.00","4.38","53.04"]
["8.1","30412227换1","金属软管敷设 DN20 ( 每根长≤\n0.5m)","m","10","30.86","10.95","0.00","0.00","4.10","2.75","0.00","4.38","53.04"]
["9","030411004003","配线\n1.管内穿线 穿照明线 铜芯 BV-2.5","m","590","0.89","2.00","0.00","0.00","0.28","0.19","0.00","0.30","3.66"]
["9.1","30413005换1","管内穿线 穿照明线 铜芯 BV-2.5","单线","590","0.89","2.00","0.00","0.00","0.28","0.19","0.00","0.30","3.66"]
["10","030411004004","配线\n1.管内穿线 穿照明线 铜芯 BV-4","m","40","0.59","2.78","0.00","0.00","0.33","0.22","0.00","0.35","4.27"]
["10.1","30413006换1","管内穿线 穿照明线 铜芯 BV-4","单线","40","0.59","2.78","0.00","0.00","0.33","0.22","0.00","0.35","4.27"]
["11","030901010002","室内消火栓\n1.更换消火栓箱门（650*800mm）","套","1","0.00","0.00","0.00","0.00","0.00","0.00","0.00","0.00","150"]
["11.1","bc0101","更换消火栓箱门（650*800mm）","套","1","0.00","0.00","0.00","0.00","0.00","0.00","0.00","0.00","150"]
["12","BC01001","消防管改接\n  1.消防管改接","项","1","0.00","0.00","0.00","0.00","0.00","0.00","0.00","0.00","800"]
["12.1","BC01","消防管改接","项","1","0.00","0.00","0.00","0.00","0.00","0.00","0.00","0.00","800"]
["13","030413002001","凿(压)槽\n  1.剔堵槽、沟 砖结构 宽mm*深\nmm (70*70)","m","20","8.77","10.70","0.00","0.00","1.91","1.28","0.00","2.04","24.7"]
["13.1","31011156","剔堵槽、沟 砖结构 宽mm*深mm \n(70*70)","m","20","8.77","10.70","0.00","0.00","1.91","1.28","0.00","2.04","24.7"]
["14","030411002001","线槽\n1.塑料线槽敷设 DN25","m","10","8.68","3.15","0.00","0.00","1.16","0.78","0.00","1.24","15.01"]
["14.1","30412244换1","塑料线槽敷设 DN25","m","10","8.68","3.15","0.00","0.00","1.16","0.78","0.00","1.24","15.01"]
[]
[null,null," "," "," "," "," "," "," "," "," "," "," "," "]

{"sheet":"表11单价措施项目清单综合单价分析表","index":8,"n_rows":61,"n_cols":13,"rows_kept":61,"merged":[[0,0,0,1],[1,0,1,12],[2,0,2,10],[2,11,2,12],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,3,11],[3,12,4,12],[7,1,7,12],[14,0,14,1],[15,0,15,12],[16,0,16,10],[16,11,16,12],[17,0,18,0],[17,1,18,1],[17,2,18,2],[17,3,18,3],[17,4,18,4],[17,5,17,11],[17,12,18,12],[20,1,20,12],[21,1,21,12],[27,0,27,1],[28,0,28,12],[29,0,29,10],[29,11,29,12],[30,0,31,0],[30,1,31,1],[30,2,31,2],[30,3,31,3],[30,4,31,4],[30,5,30,11],[30,12,31,12],[34,1,34,12],[37,1,37,12],[47,0,47,1],[48,0,48,12],[49,0,49,10],[49,11,49,12],[50,0,51,0],[50,1,51,1],[50,2,51,2],[50,3,51,3],[50,4,51,4],[50,5,50,11],[50,12,51,12],[53,1,53,12],[54,1,54,12]],"flags":["formulas_cached_only"]}
["  表11",null," "," "," "," "," "," "," "," "," "," "," "]
["单价措施项目清单综合单价分析表"]
["工程名称:三层会议室及办公室_土建单位工程",{"$nulls":10},"第1页 共4页"]
["序号","项目编码","项目名称及特征描述","单位","工程量","综合单价组成（元）",{"$nulls":6},"综合单价\n（元）"]
[{"$nulls":5},"人工费","材料费","施工机具使用费","企业管理费","利润","规费","税金"]
[" "," "," "," "," "," "," "," "," "," "," "," "," "]
[" "," "," "," "," "," "," "," "," "," "," "," "," "]
["一","其他措施项目"]
["1","011703001001","垂直运输\n  1.人工搬运 ( 各种胶合板材、\n石膏板 每上2层楼)\n  2.人工搬运 ( 门窗 每上2层楼)\n  3.人工搬运 ( 钢筋、水泥、石\n灰、油漆、涂料  每上2层楼)","项","1","585.21","0.01","0.00","56.97","39.27","0.00","60.90","742.37"]
["1.1","10117107换1","人工搬运 ( 各种胶合板材、石膏\n板 每上2层楼)","m2","192.54","2.98","0.00","0.00","0.29","0.20","0.00","0.31","3.78"]
["1.2","10117110换1","人工搬运 ( 门窗 每上2层楼)","m2","3.39","1.20","0.00","0.00","0.12","0.08","0.00","0.13","1.53"]
["1.3","10117104换1","人工搬运 ( 钢筋、水泥、石灰、\n油漆、涂料  每上2层楼)","t","0.066","111.71","0.22","0.00","10.97","7.37","0.00","11.73","142.17"]
[]
[null,null," "," "," "," "," "," "," "," "," "," "," "]
["  表11",null," "," "," "," "," "," "," "," "," "," "," "]
["单价措施项目清单综合单价分析表"]
["工程名称:三层会议室及办公室_安装单位工程",{"$nulls":10},"第2页 共4页"]
["序号","项目编码","项目名称及特征描述","单位","工程量","综合单价组成（元）",{"$nulls":6},"综合单价\n（元）"]
[{"$nulls":5},"人工费","材料费","施工机具使用费","企业管理费","利润","规费","税金"]
[" "," "," "," "," "," "," "," "," "," "," "," "," "]
["一","措施分部L01"]
["二","措施项目"]
["1","031301017001","脚手架搭拆","项","1","34.75","64.54","0.00","9.93","6.95","0.00","10.92","127.09"]
["1.1","JSJ009","消防脚手架搭拆费","元","12.378","0.35","0.65","0.00","0.10","0.07","0.00","0.11","1.28"]
["1.2","JSJ005","电气设备安装脚手架搭拆费","元","86.915","0.35","0.65","0.00","0.10","0.07","0.00","0.11","1.28"]
[]
[null,null," "," "," "," "," "," "," "," "," "," "," "]
["  表11",null," "," "," "," "," "," "," "," "," "," "," "]
["单价措施项目清单综合单价分析表"]
["工程名称:六层会议室及办公室_土建单位工程",{"$nulls":10},"第3页 共4页"]
["序号","项目编码","项目名称及特征描述","单位","工程量","综合单价组成（元）",{"$nulls":6},"综合单价\n（元）"]
[{"$nulls":5},"人工费","材料费","施工机具使用费","企业管理费","利润","规费","税金"]
[" "," "," "," "," "," "," "," "," "," "," "," "," "]
[" "," "," "," "," "," "," "," "," "," "," "," "," "]
["一","脚手架"]
["1","011701003001","砌筑脚手架\n1.里脚手架","m2","4.47","2.13","0.38","0.49","0.29","0.20","0.00","0.31","3.80"]
["1.1","10117017","里脚手架","m2","4.47","2.13","0.38","0.49","0.29","0.20","0.00","0.31","3.8"]
["二","其他措施项目"]
["1","011703001002","垂直运输\n  1.人工搬运 ( 砖、砌块、碎石\n、砂土  每上五层楼)\n  2.人工搬运 ( 钢筋、水泥、石\n灰、油漆、涂料  每上五层楼)\n  3.人工搬运 ( 各种胶合板材、\n石膏板 每上五层楼)\n  4.人工搬运 ( 门窗 每上五层楼\n)","项","1","1280.20","0.45","0.00","124.69","83.87","0.00","133.31","1622.48"]
["1.1","10117103换1","人工搬运 ( 砖、砌块、碎石、砂\n土  每上五层楼)","m3","0.14","93.97","1.84","0.00","9.39","6.31","0.00","10.04","121.55"]
["1.2","10117104换2","人工搬运 ( 钢筋、水泥、石灰、\n油漆、涂料  每上五层楼)","t","0.425","223.69","0.44","0.00","21.97","14.77","0.00","23.48","284.36"]
["1.3","10117107换2","人工搬运 ( 各种胶合板材、石膏\n板 每上五层楼)","m2","194.35","5.96","0.00","0.00","0.58","0.39","0.00","0.62","7.55"]
["1.4","10117110换2","人工搬运 ( 门窗 每上五层楼)","m2","5.7","2.39","0.00","0.00","0.23","0.16","0.00","0.25","3.03"]
["2","011703001003","垂直运输\n1.人工搬运 ( 垃圾每向下5层楼)","项","1","1019.49","5.20","0.00","100.43","67.48","0.00","107.37","1299.97"]
["2.1","10117113换1","人工搬运 ( 垃圾每向下5层楼)","m3","7.54","135.21","0.69","0.00","13.32","8.95","0.00","14.24","172.41"]
[]
[null,null," "," "," "," "," "," "," "," "," "," "," "]
["  表11",null," "," "," "," "," "," "," "," "," "," "," "]
["单价措施项目清单综合单价分析表"]
["工程名称:六层会议室及办公室_安装单位工程",{"$nulls":10},"第4页 共4页"]
["序号","项目编码","项目名称及特征描述","单位","工程量","综合单价组成（元）",{"$nulls":6},"综合单价\n（元）"]
[{"$nulls":5},"人工费","材料费","施工机具使用费","企业管理费","利润","规费","税金"]
[" "," "," "," "," "," "," "," "," "," "," "," "," "]
["一","措施分部L01"]
["二","措施项目"]
["1","031301017002","脚手架搭拆","项","1","47.25","87.75","0.00","13.50","9.45","0.00","14.85","172.81"]
["1.1","JSJ009","消防脚手架搭拆费","元","12.378","0.35","0.65","0.00","0.10","0.07","0.00","0.11","1.28"]
["1.2","JSJ005","电气设备安装脚手架搭拆费","元","113.859","0.35","0.65","0.00","0.10","0.07","0.00","0.11","1.28"]
["1.3","JSJ010","给排水、采暖、燃气脚手架搭拆费","元","8.77","0.35","0.65","0.00","0.10","0.07","0.00","0.11","1.28"]
[]
[null,null," "," "," "," "," "," "," "," "," "," "," "]

{"sheet":"表14人工、材料设备、机械汇总表","index":9,"n_rows":115,"n_cols":8,"rows_kept":115,"merged":[[0,0,0,1],[1,0,1,7],[2,0,2,5],[2,6,2,7],[36,0,36,1],[37,0,37,7],[38,0,38,5],[38,6,38,7],[72,0,72,1],[73,0,73,7],[74,0,74,5],[74,6,74,7],[108,0,108,1],[109,0,109,7],[110,0,110,5],[110,6,110,7]],"flags":["formulas_cached_only"]}
["  表14",null," "," "," "," "," "," "]
["人工、材料设备、机械汇总表"]
["工程名称：水仙药业会议室及办公室装修",{"$nulls":5},"第1页 共4页"]
["序号","工料机编码","工料机名称","规格、型号等特殊要求","单位","数量","单价","合价"]
["一"," ","人工"," "," "," "," "," "]
["1","00010040","定额人工费"," ","元","18216.41","1.0876","19812.17"]
["2","JXQTRGF","其它人工费"," ","元","82.005","1","82.01"]
["二"," ","材料"," "," "," "," "," "]
["1","01610250","铁件","综合","kg","70.344","5.044","354.82"]
["2","04010170","散装水泥","42.5","kg","19.497","0.372","7.25"]
["3","13030370","乳液型涂料"," ","kg","55.602","9.58","532.67"]
["4","13030480","腻子粉"," ","kg","297.811","2.3","684.97"]
["5","17010310","焊接钢管"," ","kg","0.039","3.901","0.15"]
["6","33010040","吊杆"," ","kg","47.834","4.96","237.26"]
["7","03030530","铝合金窗帘轨","单轨 成套","m","30.2","17.7","534.54"]
["8","03030560","铝合金窗帘盒","140宽","m","32.616","57.52","1876.07"]
["9","04030230","净干砂（机制砂）"," ","m3","0.067","97.09","6.51"]
["10","04090360","粘土膏"," ","m3","0.004","26.12","0.1"]
["11","34110080","水"," ","m3","0.965","2.91","2.81"]
["12","35030310","木脚手板","500","m3","0","2113","0"]
["13","80010490","现拌抹灰砂浆","1:2.5 M40(42.5) 砂\n子4.75mm 稠度\n50~70mm","m3","0.01","299.14956","2.99"]
["14","80010500","现拌抹灰砂浆","1:3 M30(42.5) 砂子\n4.75mm 稠度50~70mm","m3","0.018","265.66956","4.78"]
["15","80050150","现拌混合砂浆","M5(42.5)","m3","0.04","152.6382","6.11"]
["16","05050010","胶合板","5厚","㎡","4.735","14.16","67.05"]
["17","09130001","铝塑板","3厚","㎡","202.239","32.74","6621.3"]
["18","10010090","轻钢龙骨(不上人型\n)","平面600×600","㎡","184.653","24.34","4494.45"]
["19","11110001_1","塑钢双开门"," ","㎡","6.78","349.56","2370.02"]
["20","11110001_2","塑钢平开门（双层\n门）"," ","㎡","2.305","700","1613.5"]
["21","35030190","扣件"," ","个","0.015","8.55","0.13"]
["22","49010040","其他材料费"," ","元","652.728","0.92","600.51"]
["23","04130540","烧结煤矸石普通砖","240×115×53","块","104.766","0.58","60.76"]
["24","03012600","地脚螺栓"," ","套","54.438","0.95","51.72"]
["25","13350660","聚氨酯发泡密封胶","750ml/支","支","8.422","7.08","59.63"]
["26","14410090","玻璃胶","350g","支","5.027","12.96","65.15"]
[]
[null,null," "," "," "," "," "," "]
["  表14",null," "," "," "," "," "," "]
["人工、材料设备、机械汇总表"]
["工程名称：水仙药业会议室及办公室装修",{"$nulls":5},"第2页 共4页"]
["序号","工料机编码","工料机名称","规格、型号等特殊要求","单位","数量","单价","合价"]
["27","18251350","镀锌异径管箍","DN32×25","个","18.18","3","54.54"]
["28","18030370","镀锌丝堵(堵头)","DN25","个","18","1.79","32.22"]
["29","02130050","聚四氟乙烯生料带","宽20","m","11.556","0.11","1.27"]
["30","03131270","尼龙砂轮片","Φ400","片","0.27","8.88","2.4"]
["31","49010030","其他材料费"," ","%","21.912","1","21.91"]
["32","23210001_1","喷头DN25"," ","个","18.18","8","145.44"]
["33","18036360","镀锌钢管接头零件","DN25","个","8.26","1.2","9.91"]
["34","01291760","热轧厚钢板","δ8～20","kg","0.686","3.89","2.67"]
["35","24110040","压力表","0-1.6MPa","块","0.028","35","0.98"]
["36","02270270","棉纱头"," ","kg","0.336","5.48","1.84"]
["37","13090050","银粉漆"," ","kg","0.029","11.63","0.34"]
["38","03131290","尼龙砂轮片","Φ500×25×4","片","0.168","10.22","1.72"]
["39","14030100","铅油","厚漆","kg","0.085","5.62","0.48"]
["40","02290110","线麻"," ","kg","0.008","7.74","0.06"]
["41","17030050_1","钢管螺纹连接 DN25"," ","m","14.07","12.46","175.31"]
["42","03130790","冲击钻头","Φ6～8","个","0.252","5.13","1.29"]
["43","03010640","木螺钉","M2-4×6-65","个","112.32","0.06","6.74"]
["44","29110400","塑料吊线盒"," ","个","37.8","1.77","66.91"]
["45","25610120","塑料网台"," ","块","37.8","0.22","8.32"]
["46","03131360","塑料胀管","Φ6-8","个","39.6","0.04","1.58"]
["47","28031940","铜芯聚氯乙烯绝缘\n电线","BV-2.5","m","23.794","1.47","34.98"]
["48","28032110","铜芯橡皮花线","BXH 2×23/0.15","m","73.296","3.54","259.47"]
["49","25000020_1","吊顶灯600*6000"," ","套","36.36","185","6726.6"]
["50","03012440","半圆头镀锌螺栓","M2～5×15～50","个","87.36","0.35","30.58"]
["51","26050260_1","双联开关"," ","个","8.16","7.6","62.02"]
["52","01030190","镀锌铁丝","Φ2.2～1.2","kg","2.45","5.13","12.57"]
["53","03131120","钢锯条"," ","根","3.5","0.23","0.81"]
["54","14410760","粘合剂","507","kg","0.35","7.56","2.65"]
["55","29061400","难燃塑料管接头","25","个","90.3","0.27","24.38"]
["56","29060930_1","刚性阻燃管敷设 砖\n、混凝土结构暗配 \nPVC20"," ","m","371","1.13","419.23"]
[]
[null,null," "," "," "," "," "," "]
["  表14",null," "," "," "," "," "," "]
["人工、材料设备、机械汇总表"]
["工程名称：水仙药业会议室及办公室装修",{"$nulls":5},"第3页 共4页"]
["序号","工料机编码","工料机名称","规格、型号等特殊要求","单位","数量","单价","合价"]
["57","03010900","半圆头螺钉","M6～12×12～50","套","163.36","0.12","19.6"]
["58","29170150","镀锌地线夹","20","套","61.86","1.77","109.49"]
["59","18150500","金属软管接头","DN20","个","20.6","2.3","47.38"]
["60","18250280","金属软管卡","DN20","个","44","0.12","5.28"]
["61","17190001_1","金属软管敷设 \nDN20 ( 每根长≤\n0.5m)"," ","m","20.6","1.65","33.99"]
["62","27170180","电气绝缘胶带","18mm×10m×0.13mm","卷","3.23","4.42","14.28"]
["63","02270260","棉纱"," ","kg","2.22","5.29","11.74"]
["64","14030060","汽油","92#","kg","5.55","6.61","36.69"]
["65","03131890","锡基钎料"," ","kg","2.22","42.48","94.31"]
["66","28000010_1","管内穿线 穿照明线\n 铜芯 BV-2.5"," ","m","1171.6","1.6","1874.56"]
["67","28000010_2","管内穿线 穿照明线\n 铜芯 BV-4"," ","m","110","2.4","264"]
["68","26410370_2","五孔插座"," ","套","30.6","7.2","220.32"]
["69","28031970","铜芯聚氯乙烯绝缘\n电线","BV-6","m","1.22","3.41","4.16"]
["70","26410370_3","空调插座"," ","套","4.08","15","61.2"]
["71","34110030","电"," ","kW·h","2.14","0.7345","1.57"]
["72","80010040","水泥砂浆","1:3(32.5)","m3","0.1","294.0476","29.4"]
["73","010101001010","水泥","32.5(砂浆用)","kg","50.1","0.358","17.94"]
["74","04030120","中(细)砂","损耗2%+膨胀1.18","m3","0.122","145.63","17.77"]
["75","80010030","水泥砂浆","1:2.5(32.5)","m3","0.02","323.0456","6.46"]
["76","03131700","合金钢切割片","Φ300","片","0.88","195.58","172.11"]
["77","JXQTCLF","其他材料费"," ","元","152.295","1","152.3"]
["78","29030070","塑料线槽配件","断面周长120以内","个","7","1.33","9.31"]
["79","29030060_1","塑料线槽"," ","m","10.5","2.1","22.05"]
["三"," ","设备"," "," "," "," "," "]
["四"," ","机械"," "," "," "," "," "]
["1","99050210","灰浆搅拌机","拌筒容量200L","台班","0.01","136.64","1.37"]
["2","99070530","载货汽车","装载质量6t","台班","0.005","404.26","2.02"]
["3","99070610","自卸汽车","装载质量4t","台班","0.383","442.94","169.65"]
["4","99250020","交流弧焊机","容量32kV·A","台班","5.03","80.3","403.91"]
["5","99190860","管子切断套丝机","Φ159","台班","0.294","20.08","5.9"]
[]
[null,null," "," "," "," "," "," "]
["  表14",null," "," "," "," "," "," "]
["人工、材料设备、机械汇总表"]
["工程名称：水仙药业会议室及办公室装修",{"$nulls":5},"第4页 共4页"]
["序号","工料机编码","工料机名称","规格、型号等特殊要求","单位","数量","单价","合价"]
["6","99440460","试压泵","压力3MPa","台班","0.021","16.45","0.35"]
[]
[null,null," "," "," "," "," "," "]